* An AF4 data evaluation software is presented
* The comparison of AF4 channel width calibration procedures shows inconsistent results
* A deviation analysis identifies the measured void peak as an error-prone parameter
* Adjusting the measured void peak to a calculated value resolves the observed discrepancies