Highlights

* Automating of AF4 data evaluation
* Independence from signal quality in the void peak range
* Increase of the data liability
* Alternative calibration-free evaluation method
* Detailed error consideration